

**Neo Modern**



vdalve & flexible hose CCAS2074-2200400C0

Close Coupled Toilet

TF-2630



**SPECIFICATIONS**

* Flushing Type: Dual Flush 3 / 4.2 L
* Push Button: Top push
* Outlet Type: P Trap & S Trap with Plastic Connector
* Bowl Shape: Elongated
* Rough in: S-trap 305 mm., P-trap 190 mm
* Overall Dimensions: W376\*L710\*H792 mm.
* Height to rim: 390 mm.
* Material: Vitreous China

**FEATURES**

* Dual Flush Wash Down
* Water Saving
* Concealed Trapway
* Slow Closing Seat & Cover

**COLOR AVAILABILITY**

* White only(0)

**INCLUDED COMPONENTS**

* Slow Closing Seat & Cover
* Tank Fitting Set
* Connector
* L-Shape Floor Fixing
* Stop Valve
* Installation manual


**SHIPPING WEIGHT**



* Net Weight: 42.0 KGs.
* Gross Weight:

**STANDARD CRITERIA**

* TIS-792:2554\_2011
* PNS-993-2010
* MS 1522-2011
* SS 378-1996
* GB 6952-2005

**DIMENSIONAL DRAWING**



This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.