

**Acacia Evolution**



One-Piece Toilet

TF-2007

\\ranthfs001\lixilasean\4_Product_Pictures\1_VC\VC\HiRes\Toilet\Acacia Evolution\acaciaE OP toilet (TF-2007).tif

**FEATURES**

Double Vortex Wash Down

Anti – Bacteria on Push Button & Seat & Cover.

Proguard

Technology

Water Saving

Rimless

Easy to Clean

Slow Closing Seat & Cover

**SPECIFICATIONS**

Flushing Type: Dual Flush 2.6/4 Litres per flush

Push Button: Top push

Outlet type: P-trap & S-trap with Plastic Connector

Bowl shape: Elongated

Roughing in: S-trap 305 mm., P-trap 190 mm

Overall Dimensions: W376xL740xH654 mm.

Height to rim: 390 mm.

Material: Vitreous China

**COLOR AVAILABILITY**

White (WT)

**INCLUDED COMPONENTS**

Slow closing seat & cover

Dual tank fitting set

S-trap connector

L-shape floor fixing set

Plastic side cover

Stop valve

Installation manual

**SHIPPING WEIGHT**

Net weight: 49.2 KGs

Gross weight: 58.7 KGs

**STANDARDS CRITERIA**

TIS-792:2001

GB 6952-2005

PNS 156:2010

MS 1522:2007

SS 378-1996

ASME-A112.19.2-2008

**DIMENSIONAL DRAWING**







This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.