

**CODIE**



Exposed Bath & Shower Mixer with Handshower

**STANDARD SPECIFICATION**

* Chromium plating for durable finish
* Ceramic disc cartridge
* Strong brass construction
* Wall-mounted installation
* Exposed aerator
* With 3-function handshower set

1) Spray; 2) Massage; 3 Spray+Massage

* Flow rate @ 0.1 MPa (with spout) 10.56 L/min
* Flow rate @ 0.1 MPa (with handshower) 6.48 L/min
* Spout reach : 111 mm

**PRODUCT WEIGHT:** 2.43 **Kg**

**APPLICABLE CODES & STANDARDS:**

* TIS 2067-2552
* GB 18145-2014

**STANDARDS CRITERIA**





