

**CODIE**



Single-hole Basin Mixer without Pop-up Drain

FFASB201-101501BF0

**STANDARD SPECIFICATION**

* Chromium plating for durable finish
* Ceramic disc cartridge
* Strong brass construction
* Single-hole installation
* Exposed aerator with 15o
* Flow rate @ 0.1 MPa (3.24 L/min)
* Spout reach : 110 mm
* Spout height : 75 mm

**PRODUCT WEIGHT: 1.58 Kg**

**APPLICABLE CODES & STANDARDS:**

* TIS 2067-2552
* GB 18145-2014

**STANDARDS CRITERIA**



