

**Acacia SupaSleek**



BTW Toilet

CL3229

**FEATURES**

Double Vortex Wash Down

Aqua Cermaic&Comfort Clean

Water Saving



Rimless

CrystaSleek Seat & Cover

**SPECIFICATIONS**

Flushing Type: Dual Flush 3/4.5 Litres per flush

Tank Fitting: Concealed cistern

Outlet type: S-trap & P-trap

Bowl shape: Elongated

Overall Dimensions: W376xL555xH390mm

Height to rim: 390 mm.

Material: Vitreous China

**COLOR AVAILABILITY**

White (WT)

**INCLUDED COMPONENTS**

L-shape floor fixing set 80 mm

Installation manual

**SHIPPING WEIGHT**


Net weight: 31 KGs


Gross weight: 34.4 KGs

**STANDARDS CRITERIA**


TIS-792:2001


**DIMENSIONAL DRAWING**

S-trap



P-trap





This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.