

**Concept Nuovo**



vdalve & flexible hose CCAS2074-2200400C0

Wall Hung Bowl

TF-3105

 

**SPECIFICATIONS**

* Flushing Type: Dual Flush 3 / 4.5 L
* Tank Fitting: Concealed cistern
* Outlet Type: P-trap
* Bowl Shape: Round Bowl
* Overall Dimensions: W365\*L560\*H352 mm.
* Material: Vitreous China

**FEATURES**

* Dual Flush Wash Down
* Water Saving
* Slow Closing Seat & Cover

**COLOR AVAILABILITY**

* White only(0)

**INCLUDED COMPONENTS**

* Installation Manual

**SHIPPING WEIGHT**

* Net Weight: 28.25 KGs
* Gross Weight: 31 KGs.

**STANDARD CRITERIA**

* TIS-792:2554\_2011
* PNS-993-2010
* ASME-A112.19.2-2008

**DIMENSIONAL DRAWING**



This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.