

**CODIE**



Exposed Shower Mixer without Handshower

**STANDARD SPECIFICATION**

* Chromium plating for durable finish
* Ceramic disc cartridge
* Strong brass construction
* Wall-mounted installation
* Flow rate @ 0.1 MPa (without handshower) 14.76 L/min

**PRODUCT WEIGHT:** 1.85 **Kg**

**APPLICABLE CODES & STANDARDS:**

* TIS 2067-2552
* GB 18145-2014

**STANDARDS CRITERIA**



